### Demonstration Spiel for Silent Sound Demo Device
September 28, 2000

    ===========================================================================

                    DEMONSTRATION PROCEDURES

    1.  THOROUGHLY go through the setup procedures first.  You need to be
        completely familiar with the unit before attempting to demonstrate
        it to the public.  Be sure your battery has been charged overnight.

        Setup procedures

    2.  Shortly before the demo, refresh yourself on:

        - U.S. Govt (NSA) admission mind control exists nsa1.gif
        - unclassified and commercial mind-weapons-capable devices uncom.htm
        - MKULTRA and the successful lawsuit against the CIA anat-1.htm

    3.  MATERIALS.  You need, when dealing with the public:

        - a printout of THIS SET OF INSTRUCTIONS
        - a printout of hypno2s.gif (see other below)
        - a printout of mkcover.gif (OPTIONAL)
        - a picket sign (if outdoors without a pre-arranged meeting with visitors)
        - some handouts, one sheet of which MUST be nsa1.gif
          (This has proven very compelling to those who read it)
        - for YOUR reference, a printout of Judy Wall's article
          on silent sound, including Gulf War use, silsoun2.htm
        - a copy of these instructions and spiel script
        - small flip-nozzle container of water for your voice and
          perhaps throat lozenges
        - sunscreen and sun hat if outdoors
        - a small tape recorder with a voice-ONLY cassette, normal sound
        - a patch cord between the "ear" jack on the recorder and the
          MONO 1/8" jack on the demo unit (keep volume low or use an
          attenuator from Radio Shack. Excess volume results in garble.)

        Some may find this image explaining silent sound WITHOUT the
        extra clutter from the voice-to-skull attachment easier to use:
        - a printout of voicefm.gif (OPTIONAL)

        Some may wish to hand out schematics.  I recommend this schematic
        and matching solder-side component placement image:
        - vfmckt3.gif, schematic
        - kitbotm3.gif, solder-side layout

    4.  ICE-BREAKER.  Mine is a picket sign that carries this message:

        "GOVT-MEDIA  TELL THE PUBLIC  ABOUT ELECTRONIC MIND WEAPONS"

        poster9.gif

    5.  SPIEL.  The words below VARY according to the person I'm talking
        with, and for best effectiveness you will need to judge just how
        interested the visitor is.  I've had SHORT visits like:

        VISITOR:  What is this? (Pointing to the demo unit)

        DEMONSTRATOR:  This is a device which takes ordinary human speaking
        voice and does two things to it:

        - converts it from natural AM (amplitude modulation) to FM
          (frequency modulation); this garbles the voice
        - raises the average frequency from around 1,500 Hertz, which
          is normal, to around 15,000 Hertz.

        At 15,000 Hertz, young people with good hearing can hear a
        slight "ringing in the ears" from this device, while many adults
        hear nothing at all.

        But the brain CAN HEAR THE WORDS, even though the ear cannot.

        This allows a hypnotist to program an individual over months and
        years without the target being aware.  There is no resistance to
        the hypnosis because the target doesn't hear it.

        This can be beneficial, but it can also do severe damage to a
        person's well being.  This is why our group is out here demonstrating.

        We want government to earn their salaries and perks by placing controls
        on who can possess such devices and what can be legally done with them.

        VISITOR:  Thank you (and leaves.)

        >> LONG visits start out as above.  If questions keep coming, you will
        need to answer them.  Below are some typical questions and answers:

        DEMONSTRATOR:  (Continuing from the "short" spiel above)

        ** AT THIS POINT, YOU MAY WANT TO DROP DOWN THIS SCRIPT TO ITEM #6,
           THE ACTUAL PHYSICAL DEMO OF THE UNIT.  I HAVE FOUND THAT A GREAT
           MANY VISITORS DO NOT WANT TO HEAR THE UNIT.  I NEVER PRESS THAT
           ISSUE WITH THEM, AND ONLY START IT UP WHEN ASKED.

        This device as it is here is harmless, unless used on someone who has
        already been programmed with trigger words or phrases.  It becomes
        very invasive and dangerous, though, if connected to a voice-to-skull
        projector.  A voice-to-skull projector is a modified radar transmitter
        in which the human voice controls how close together the radar pulses
        occur.

        In 1974, Dr. Joseph Sharp, of the Walter Reed Army Institute of
        research, announced his successful transmission of speech directly
        into the human skull with no receiving device.  By connecting this
        "silent sound" device to a voice-to-skull transmitter, it is possible
        to transmit hypnotic phrases silently into a target's bedroom,
        every night, for years, without the target's being aware.

        By programming enough "Pavlovian triggers" into an individual, that
        individual's personality can be changed substantially.

        Using pre-programmed trigger phrases, a "handler" of that individual
        can literally use him or her as a "living robot", in cases where the
        individual has high susceptibility to hypnosis.

        The process of programming enough triggers into an individual for
        purposes of control is called "creating a Manchurian Candidate", after
        two books of that title.

        The formal program of the CIA, begun in the 1950s, started out as
        149 separate experiments, and was in response to cold war fears and
        the apparent "brainwashing" of Allied POWs in Korea.  This group
        of "behaviour modification" experiments bore the code name MKULTRA.

        MKULTRA did include electronic mind control devices, but the best
        known electronic mind control device of the early days was the
        Russian LIDA machine.  The LIDA, one of which is in possession of
        Veterans' Administration researcher Dr. Ross Adey, "entrained" or
        electronically coerced a target in the path of it's signal to be
        relaxed and more susceptible to hypnosis.  A few Korean War vets
        claimed to have seen the LIDA in use at the POW camps.

        The MKULTRA code name ceased in the late 1970s when the U.S. Senate's
        Frank Church Committee investigated MKULTRA experiments and found that
        serious atrocities had been committed on people in the military,
        prisons, or in mental hospitals.  However, not one single perpetrator
        from the MKULTRA programs was ever brought up on charges.

        We know that electronic mind control experimentation did not cease,
        and this "silent sound" technology was used in actual military
        combat in the 1991 Gulf War.  The United States Army connected
        a silent sound voice converter like this one to an FM broadcast
        transmitter, broadcasting on a frequency of 100 Megahertz, and the
        silent hypnotic commands were carried right on top of normal voice
        in the Iraqi language.  The normal voice carried confusing information,
        while the SILENT component re-inforced a sense of despair by hypnotic
        suggestion.

        This was documented on Britain's ITV network, but not shown in the
        U.S. or Canada.

        The successful use by the U.S. Army clearly shows that this technology
        does work.  Through-the-wall voice-to-skull technology makes it almost
        inescapable.  Our group hopes that eventually the public will learn
        enough about the invasive privacy destroying electronic mind control
        weapons available today to demand that government report on these
        devices to the people, and make their use and possession matters of
        ongoing PUBLIC record.

        Electronic mind control devices have been under development for 50
        years, and our group knows only the unclassified and commercial
        versions.  The time for public input and control of all such
        techologies is LONG overdue.

    6.  ACTUAL DEMONSTRATION OF THE UNIT ITSELF.

        Put a tape with VOICE (not music) into your demo tape recorder.

        Connect a patch cable between the "ear" jack on the recorder and
        the INPUT jack on the demo unit.  If you have an attenuator, use
        it, but if not, remember to keep the volume setting on the recorder
        quite low.  Excess volume garbles the speech making for an un-
        convincing demo.

        Switch on the demo unit.  Adjust the tone near the lower end of
        the frequency knob's travel.  The Input Level should be around
        one third of it's way up from it's lowest position.

        Push PLAY on the recorder.  You should hear speech "mixed" in with
        the demo unit's tone.  This demonstrates to a visitor what simply
        converting natural human voice, which is AM or amplitude modulation
        to FM or frequency modulation sounds like.  Near the low end of the
        frequency knob's travel, the frequencies of the voice are still
        about at their natural values, but the mode is now FM, as opposed
        to AM.  THE VISITOR CAN HEAR THIS IS GARBLED.

        Now slowly increase the frequency knob until the audible sound
        is as HIGH as you and your visitor can just hear.  If you are both
        adults, this point is approximately where the brain can start to
        convert this inaudible sound BACK TO WORDS.  The process is called
        "slope tuning".  You can move the IN-OFF-OUT switch back to IN to
        show the visitor that voice is actually being fed into the unit.

        vfmslopd.gif, shows how the brain recovers
        the inaudible words using the process of "slope detection" or "slope
        tuning" - worth having a few of these for technical folks who are
        interested in how it works.

        If you have a frequency counter or meter, connect it to the two
        binding posts, one red, one black, on the front panel.  During
        a demo adjust frequency somewhere between 14.5 and 14.8 kHz
        (14,500 Hertz to 14,800 Hertz.)  This is the range where both
        the Lowery patent (5,159,703) and the New Zealand Altered States
        company operate at to produce brain-understandable silent sound.

        >> SEE ITEM 4 BELOW UNDER SETUP FOR COMMENTS ABOUT USING AN AUDIO
           LEVEL METER TO ENHANCE YOUR DEMONSTRATION

    ===========================================================================
    Back to top

                           SETUP PROCEDURES

    vfmtest.gif, shows what the scope trace
    should look like when proper frequency modulation by voice is applied.

    vfmslopd.gif, shows how the brain recovers
    the inaudible words using the process of "slope detection" or "slope
    tuning" - worth having a few of these for technical folks who are
    interested in how it works.

    1.  You will need a small voltmeter to monitor battery charge state.
        This must be a small meter that reads out VOLTS, and *NOT* a
        "battery OK" meter with red and green scales.  It is necessary
        to know voltages for communications by email or phone with
        people who can offer technical help.

        A convenient meter is the Radio Shack 22-802, for around $30,
        which has a folding case fully containing the two probes and
        their cable.  The only trick with any meter is TO REMEMBER
        TO SHUT IT OFF WHEN YOU ARE FINISHED.  Almost all of today's
        voltmeters have digital displays and have their own small
        internal battery.  (Pick up and carry a spare battery.)

    2.  First job is to charge the internal 12-volt gel cell.

        The charger supplied with units purchased from Eleanor White
        is a simple "wall mount" style 12-volt power supply, with a
        cable that cannot be connected with the wrong polarity.

        Measure the voltage by touching the positive (red lead) screw
        on the terminal strip with the red probe, and the negative
        (black lead) screw on the terminal strip with the black probe.

        You should get "13 something" volts if the battery is reasonably
        well charged.  If you get zero volts, it is likely that one of
        the 3/4 amp fuses is blown.  Check both fuses to be sure.

        (You can check a fuse visually, but 3/4 amp size is hard to see.
        Instead, switch your meter to K-ohms and put the probes on either
        end of the glass fuse.  The fuse should show zero or very close
        to zero if it is good.  The fuses are 5 MILLIMETER and you may
        need to go to Radio Shack to get replacements.

        !!!!! SWITCH YOUR METER OFF OR BACK TO VOLTS WHEN FINISHED !!!!!

        Now remove the probes and connect your charger.  Put the probes
        back on their screws and note the voltage reading.  If charging
        is in progress, you should see "14 something" volts and perhaps
        as high as 15 volts.  If you don't, something is wrong - see the
        paragraph on blown fuses above, or be sure the charger is plugged
        in, or be sure the outlet has power.

        If your "wall mount" power supply has a SLIDE SWITCH TO CHANGE
        VOLTAGE, be sure it is set to "12".

    3.  Switch the unit on.  You should see the LED on the panel lit up.
        If not, check the fuses.

        Switch the IN-OFF-OUT switch to OUT.  Turn the frequency control
        to the lower part of its travel.  Be sure the Output Level knob
        is at least 1/4 of the way up.  You should hear a steady tone.

        Test that the frequency control can raise the tone high enough
        that you can no longer hear it, then bring it back down low.

        Switch the IN-OFF-OUT switch to IN.  Raise the Input Level to
        full scale.  If you get a squeal, as sometimes happens with
        PA systems, you need to make a mental note of where that
        occurs and not go above that point with INPUT level.

    4.  Put a tape with VOICE (not music) into your demo tape recorder.

        >> COMMENTS ABOUT AUDIO LEVEL METER DEMOS ARE AT THE END OF THIS ITEM.

        Connect a patch cable between the "ear" jack on the recorder and
        the INPUT jack on the demo unit.  If you have an attenuator, use
        it, but if not, remember to keep the volume setting on the recorder
        quite low.  Excess volume garbles the speech making for an un-
        convincing demo.

        Switch on the demo unit.  Adjust the tone near the lower end of
        the frequency knob's travel.  The Input Level should be around
        one third of it's way up from it's lowest position.

        Push PLAY on the recorder.  You should hear speech "mixed" in with
        the demo unit's tone.  This demonstrates to a visitor what simply
        converting natural human voice, which is AM or amplitude modulation
        to FM or frequency modulation sounds like.  Near the low end of the
        frequency knob's travel, the frequencies of the voice are still
        about at their natural values, but the mode is now FM, as opposed
        to AM.  The visitor can hear this is garbled.

        Now slowly increase the frequency knob until the audible sound
        is as HIGH as you and your visitor can just barely hear.  If you
        are both adults, this point is approximately where the brain can
        start to convert this inaudible sound BACK TO WORDS.  The process
        is called "slope tuning".  You can move the IN-OFF-OUT switch back
        to IN to show the visitor that voice is actually being fed into
        the unit.

        If you have a frequency counter or meter, connect it to the two
        binding posts, one red, one black, on the front panel.  During
        a demo adjust frequency somewhere between 14.5 and 14.8 kHz
        (14,500 Hertz to 14,800 Hertz.)  This is the range where both
        the Lowery patent (5,159,703) and the New Zealand Altered States
        company operate at to produce brain-understandable silent sound.

        If you have an AUDIO LEVEL METER, it can be used to show that
        sound is coming out at 14.5 kHz even though it is inaudible.

                          !!!!! BUT BEWARE !!!!

        Some audio meters like Radio Shack's CUT OFF AT OR NEAR 20 kHz.

        You need to do considerable testing in private before you attempt
        audio meter proof in front of visitors.  It is quite easy to get
        the frequency too high, in which case the audio level meter will
        show nothing at all.

        To be practical, you really would need a frequency meter connected
        to the binding posts to assure yourself you were in the 14.5-14.8
        range.

        Furthermore, the piezo tweeter is good at high end frequencies,
        but the common audio chips in the unit are not really strong at
        these high-end frequencies.  If you plan to use an audio level
        meter, I'd recommend something like the Radio Shack amplified
        speaker, catalogue #21-541, requiring it's own separate 12-volt
        source (the demo unit's can be tapped by someone with electronic
        assembly skills.  This will shorten the charge life of the demo
        unit's battery but may be worth doing anyway.)

        If you do use an external amplifier, be SURE it gets it's normal
        voice coil speaker replaced with a PIEZO unit or the high freq-
        uency sound won't get through well enough for the audio level
        meter to detect.

    ===========================================================================
    Back to top

ALPHABETICAL Site index page
SUBJECT Site index page